

Packet Tracer - Configure Dynamic NAT

Nombres: Brayan Ortiz Cundar, Luis Pérez Señalin y Jossué Rivadeneira Ordóñez

# Objectives

**Part 1: Configure Dynamic NAT Part 2: Verify NAT Implementation**

# Instructions

**Part 1: Configure Dynamic NAT**

## Step 1: Configure traffic that will be permitted.

On **R2**, configure one statement for ACL 1 to permit any address belonging to the 172.16.0.0/16 network.

## Step 2: Configure a pool of address for NAT.

Configure **R2** with a NAT pool that uses two addresses in the 209.165.200.228/30 address space.

Notice in the topology there are 3 network addresses that would be translated based on the ACL created. What will happen if more than 2 devices attempt to access the internet?

**R:** The first and second devices will access to internet and the third devices not.

## Step 3: Associate ACL 1 with the NAT pool.

Enter the command that associates ACL 1 with the NAT pool that you just created.

## Step 4: Configure the NAT interfaces.

Configure **R2** interfaces with the appropriate inside and outside NAT commands.

Interfaz de usuario gráfica, Texto, Aplicación, Correo electrónico

Descripción generada automáticamente

# Part 2: Verify NAT Implementation

## Step 1: Access services across the internet.

From the web browser of **L1**, **PC1**, or **PC2**, access the web page for **Server1**.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

## Step 2: View NAT translations.

View the NAT translations on **R2**. Identify the internal source address of the PC and the translated address from the NAT pool in the command output.

R2# **show ip nat translations**

**Interfaz de usuario gráfica, Aplicación

Descripción generada automáticamente**

**ScreenShot:**

**Interfaz de usuario gráfica, Aplicación, Word

Descripción generada automáticamente**

 2013 - 2024 Cisco and/or its affiliates. All rights reserved. Cisco Public Page **1** of **1** [www.netacad.com](http://www.netacad.com/)